# ID 110138

Filter time for "handwheel" operation mode exceeds limit.
Description | For manual mode in handwheel operation mode, the parameter P-AXIS-00069 sets the number of CNC cycles which are used to obtain a mean value for hand wheel increments. The filter time is limited to the permissible maximum value.
Response | Class | 1 | None.
Solution | Class | 1 | Set the filter time to smaller than maximum value.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [1 µs]
Current filter time P-AXIS-00069.
%3: | Upper limit value [1 µs]
Corrected filter time P-AXIS-00069.
%4: | Corrected value [1 µs]
Error type | 2, Error message on data transfer of parameter lists to controller.