# ID 110351

Max. of vel. for axis, which is not referenced, greater than max. vel.
Description | The maximum velocity P-AXIS-00268 for the non-homed axis is greater than the maximum axis velocity.
Response | Class | 1 | Value is limited by maximum velocity.
Solution | Class | 1 | Correction of the parameter list.
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [1µm/s or 0,001°/s]
P-AXIS-00268
%3: | Limit value [1µm/s or 0.001°/s]
P-AXIS-00212
%4: | Corrected value [1µm/s or 0,001°/s]
P-AXIS-00268
Error type | 2, Error message by data transfer from parameter list into control device.