# ID 150104

Element adr_hr_zaehler in HAND_MDS greater than HLI array for hand increments.
Description | The manual mode parameters are read and interpreted by the CNC. There CNC detects that value of manual operation parameters P-MANU-00004 exceeds CNC system internal limit. Parameter P-MANU-00004 indicates the address at which the handwheel counters are sent to the CNC. In the case of the message, the high-level interface to the PLC was defined as the transfer location (see P-MANU-00003). Which area of interface is selected to give counter reading of handwheel is fixed by parameter P-MANU-00004 .
Response | Class | 3 | Manual mode parameters are not transferred to the CNC.
Solution | Class | 6 | Correction of the value for P-MANU-00004, P-MANU-00004 <= the limit value (see parameter 2 of the message). Reinterpret manual mode parameters by restarting CNC System.
Parameter | %1: | Current value [-]
Index of interface to give counter reading of handwheel to CNC which is set within manual mode parameter data set.
%2: | Limit value [-]
Maximal allowed index value.
%3: | Logical control element number [-]
Number of logical input device which parameters lead to that message.
Error type | 2, Error message by data transfer from parameter list into control device.