# Identification code for absolute path measurement system (P-AXIS-00014)

P-AXIS-00014 | Identification code for absolute path measurement system
Description | If an absolute path measurement system is used, then the parameter must be set to 1. So no homing is necessary.
Parameter | kenngr.abs_pos_gueltig
Data type | BOOLEAN
Data range | 0/1
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 0
drive types. | Simulation, SERCOS,
Remarks |