# ID 21254

Axis index is out of data format.
Description | The axis exchange command is programmed with an axis index which exceeds the permissible value range.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the axis exchange command.
Parameter | %1: | Error value [-]
Wrong index of the axis in the axis exchange command. [CHAN//section: Configuration of the path axes]
%2: | Lower limit value [-]
%3: | Upper limit value [-]
Maximum permissible axis index in channel. Version-specific setting [SYSP].
%4: | Logical axis number [-]
Logical axis number of the axis with wrong index. P-AXIS-00016, P-CHAN-00035
Error type | 1, Error message from NC program.