# ID 13208

Angle of the workpiece (@P11) and several measuring points are specified. Angle is measured.
Description | Both the angle of the workpiece edge (@P11) and more than one measuring point in the y direction (@P8) are specified. The y direction is measured and the angle is calculated from the two measured straight lines. The specified angle is not used.
Response | Class | - | Warning, cycle is continued with default value.The parameter@ P11 is ignored.
Solution | Class | - | Check parameter setting and correct input parameters.
Error type | 1, Error message from the NC program