# ID 13187

Measured radii for S0 and S180 are different
Description | The measured spindle adjusting ring radii S=0 and S=180 are different and the difference is greater than the maximum permissible deviation @P5 or, if it was not parameterised, it is greater than 0.05mm. The measurement is not reliable.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check the probe and ring for soiling and clean if necessary.Check ring attachment to the table. Check the probe or probe tip attachment.
Error type | 1, Error message from the NC program