# Parameters for Volumetric Compensation (vol_comp[i].*)

For every controller, up to five records of compensation settings can be configured. Configuration of more than only one compensation makes sense on multi-channel machines, for example.

Structure name | Index
vol_comp[i] | i = 0 ... 5

## Additional information

- Number of records to be read in (P-STUP-00100)
- Configuration file for Volumetric Compensation (P-STUP-00101)