# Segmentation specification (P-CHAN-00134)

P-CHAN-00134 | Segmentation specification (HSC)
Description | This parameter determines whether linear blocks are generated continuously, i.e. with equal segment lengths, or whether the special segmentation specification as per P-CHAN-00133 is applied.
Parameter | hsc.gen.linear_continuous_split
Data type | BOOLEAN
Data range | 0: Special segmentation specification as per P-CHAN-00133 is active. 1: Continuous block segmentation, all segments are of identical length.
Dimension | ----
Default value | 0
Remarks |