# ID 110602

Weighting factor for velocity of distance control for downward movement exceeds maximum permissible value.
Description | The velocity (P-AXIS-00415) used for the lowering movement of the distance control (see FCT-M3) can be weighted with the parameter P-AXIS-00533 ) in per mille [0.1 %]. However, the given weighting factor is greater than permissible.
Response | Class | 1 | Warning, weighting factor for velocity P-AXIS-00533 is corrected.
Solution | Class | 1 | Correct parameter P-AXIS-00533.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Error value [0,1%]
Invalid weighting value P-AXIS-00533
%3: | Upper limit value [0,1%]
Maximum permissible speed weighting P-AXIS-00533
%4: | Corrected value [0,1%]
Corrected value for speed weighting P-AXIS-00533
Error type | 2, Error message by data transfer from parameter list into control device.