# ID 50454

Clearing of backward motion memory not possible during backward motion.
Description | In the backward motion function on the path, the signal in the bahn_mc_control.backward_storage_off.command_w control unit was activated to clear the memory for backward motion. This is not possible when backward motion is active. The backward motion memory is not cleared.

For more information on backward motion [FCT-C7// Section : Forward/backward motion on the path]

Response | Class | 1 | None.
Solution | Class | 1 | Do not set the PLC signal bahn_mc_control.backward_storage_off.command_w when path motion is active.
Error type | -