# ID 150047

Axis number is 0 in continuous jog mode.
Description | The NC channel is in manual mode and an axis is to move in continuous jog mode. Continuous jog mode must be enabled for the axis and linked to a key. Select the axis by specifying its logical axis number (P-AXIS-00016). When the CNC accepts the data, it detects that the logical axis number is 0. This value is not permitted for logical axis numbers.
Response | Class | 1 | Warning
Solution | Class | 1 | Indicate the logical axis number parameterised in the axis machine data record.
Parameter | %1: | Logical axis number [-]
Incorrect logical axis number 0.
Error type | -