# ID 60208

Measure abort can not be retriggered.
Description | The abort of measuring process (PLC-block MC_AbortTrigger) was commanded while an abort of a measuring process was already active.
Response | Class | 6 | PLC module reports an error.
Solution | Class | 6 | Command abort only when previous abort is complete.
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle.
%2: | Current value [-]
Measuring channel for which abortion was commanded.
Error type | -