# ID 70310

Activation of leadscrew error compensation not possible since it is not selected in axis parameter list.
Description | To turn on leadscrew error compensation in the NC program for an axis, it must be activated in the axis parameter list (see P-AXIS-00175). See [FCT-C5// Section: Leadscrew error compensation]
Response | Class | 7 | Stop axis, leadscrew error compensation remains inactive
Solution | Class | 6 | Activate leadscrew error compensation (see P-AXIS-00175)
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected
%2: | Error value [-]
Parameter value P-AXIS-00175 to activate leadscrew error compensation
Error type | 11, Error message from position controller.