# Path velocity limit (P-CHAN-00090)

P-CHAN-00090 | Path velocity limit
Description | If no change is made to the parameter values by NC programming, this value limits path velocity after it is activated in the NC program.
Parameter | vector.velocity
Data type | REAL64
Data range | 0 ... Maximum acceleration, application-specific
Dimension | mm/min
Default value | 2000000000
Remarks | Parameterisation example: vector.velocity 1500