# ID 294045

Encoder cable failure external.
Description | Encoder cable external position input defective. Loose connection. Supply voltage missing. Encoder defective.
Response | Class | 7 | Dynamic braking. All active commands inhibited. Output $ALARM_STOP has signal level 0.
Solution | Class | 6 | Check encoder cable. Check connections. Check supply voltage. Check encoder and exchange if necessary.
Error type | 11, Error message from position controller.