# ID 110118

No measurement method was defined.
Description | If the axis is marked as a measurement axis P-AXIS-00118, a measurement method must also be parameterised. The parameter P-AXIS-00117 is set to 1.
Response | Class | 1 | None.
Solution | Class | 1 | Depending on the drive type P-AXIS-00020, at least one measurement method must be parameterised or P-AXIS-00118 must be set to 0.
Parameter | %1: | Logical axis number [-]
Logical axis number of axis affected P-AXIS-00016.
%2: | Corrected value [-]
Current drive type P-AXIS-00020.
%3: |
Corrected parameter P-AXIS-00117.
Error type | 2, Error message on data transfer of parameter lists to controller.