# ID 120690

Motion path leaves work area. PCS coordinates.
Description | Start point or target point of programmed movement path is out of active workspace. A workspace must not be left from a tool centre point. A work area can consist of an circular or polygonal area with constant third plane. See also FCT-C14. This is a subsequent error message from P-ERR-120486. It is output if the workspace is left when Cartesian transformation #(A)CS is active. The message contains the start, target point and the violating point, where the movement path enters the protection area in PCS coordinates.
Response | Class | 6 | Stop all axes immediately
Solution | Class | 6 | Dependence defined, activated work spaces
Parameter | %1: | Identification number [-]
Area Id number of left work area.
%2: | Current value [-]
Start point of movement in PCS coordinate system.
%3: | Initial value [0.1 µm or 0,0001°]
Target point of movement in PCS coordinate system.
%4: | Initial value [0.1 µm or 0,0001°]
Intersection of the motion path when leaving the workspace in the PCS coordinate system.
%5: | Error value [0.1 µm or 0,0001°]
Error type | 1, Error message from NC program.