# ID 110608

The process data for the 'value_latched' signal was not found in the cyclic process data.
Description | When configuring the SERCOS realtime status bits for the signal 'measuring probe ½', the process data element configured in P-AXIS-00677 (probe 1) or P-AXIS-00683 (probe 2) was not found in the configured cyclic process data.
Response | Class | 1 | Output of an error message containing the axis parameters P-AXIS-00118 (measurement axis) and P-AXIS-00098 (kasto_achse) are reset, in order to prevent the execution of measurement run or edge bending with incompletely configured probes.
Solution | Class | 1 | P-AXIS-00677/ or P-AXIS-00683 must be corrected.
Parameter | %1: | Logical axis number [-]
Log. Axis number
%2: | Error value [-]
Incorrect value of P-AXIS-00677/or P-AXIS-00683
%3: | Lower limit value [-]
Drive type
%4: | Upper limit value [-]
Error type | 2, Error message by data transfer from parameter list into control device.