# ID 110675

The configured bit in P-AXIS-00815 is not supported.
Description | The parameterised bit in “antr.probe_actuated_bit” () to monitor the measurement status is not supported.
Response | Class | 1 | Warning output; the value is reset. Monitoring via the HLI is not supported
Solution | Class | 1 | Bit 6/7 must be parameterised for CANopen, see
Parameter | %1: | Logical axis number [-]
Logical axis number (Axis parameters) of the drive
%2: | Current value [-]
Incorrectly parameterised value for
%3: | Corrected value [-]
Corrected value for
Error type | -