# ID 70267

Timeout while reading absolute position from drive.
Description | When requesting the absolute position from an PROFIDRIVE, the value was not delivered within the timeout limit.
Response | Class | 5 | Immediate stop of the axis.
Solution | Class | 6 | Consult drive manufacturer's documentation Check drive parameters Is the drive able to deliver absolute positions?
Parameter | %1: | Logical axis number [-]
Logical axis number of affected gantry axis see P-AXIS-00016
%2: | Current value [-]
Value of encoder state word GX_ZSW.
%3: | Upper limit value [µs]
Time-outs.
Error type |