# ID 70383

The scaled limit value is bigger than the maximum value of the configured data type.
Description | The scaled (see P-AXIS-00401) value of parameter P-AXIS-00409 is greater than the maximum value of the data type set with parameter P-AXIS-00399.
Response | Class | 1 | Warning output, P-AXIS-00409 is automatically limited to the maximum value according to P-AXIS-00399.
Solution | Class | 1 | P-AXIS-00409 value must be adjusted.
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
Value of P-AXIS-00396 for identification of drive function.
%3: | Error value [-]
Parameterized value of P-AXIS-00409.
%4: | Current value [-]
Scaling factor (see P-AXIS-00401).
%5: | Limit value [-]
Maximum possible value for P-AXIS-00409 considering P-AXIS-00399 and P-AXIS-00401 simultaneously corrected value.
Error type | 11, Error message from position controller.