# ID 70084

Plausib. error in leadscrew error compensation at inversion of direction.
Description | Plausibility error on direction reversal in leadscrew error compensation. See also [FCT-C5// Section: Leadscrew error compensation]
Response | Class | 7 | Closed-loop controlled axis stop
Solution | Class | 6 |
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis see P-AXIS-00016
%2: | Drive type [-]
Drive type of concerned axis, see P-AXIS-00020
%3: | Block number [-]
Block number of the NC program, in which the error occurred
%4: | Current value [-]
Command value
%5: | Current value [-]
Error type | 11, Error message from position controller.