# ID 20692

Select TRC in additive current interface. Channel buffers blocks.
Description | In additive current interface, the tool radius compensation is selected with G41 or G42. Because of that, all following motion blocks instructed in manual block mode are buffered by TRC and executed with delay.
Response | Class | 1 | Continue NC program processing.
Solution | Class | 1 | If possible, avoid selecting TRC while active additive current interface.
Error type | -