# Process

1. The reference tool moves to the configured starting point of the measurement in Z.
2. The reference tool is positioned simultaneously in the X and Y directions above the configured focal point of the laser.
3. The focal point of the laser is determined in the Z direction at a higher measuring speed. (when length measurement is active)
4. A precision measurement is executed in the Z direction at a slow measuring speed. (when length measurement is active)
5. The reference tool is positioned next to the laser and lowered. (when radius measurement is active)
6. A lateral measurement in XY is executed. (when radius measurement is active)
7. The reference tool is returned to the starting point position.