# ID 21215

In use of the #ECS command it is detected, that the necessary channel parameters are wrongly configured.
Description | When using the #ECS command, the program detects that the required channel parameters are incorrectly configured.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Correct setting of the ECS parameters in the channel parameter list: kind_of_2nd_ecs_ax[0] (P-CHAN-00031) mach_plane_of_2nd_ecs_ax[0] (P-CHAN-00050) Reinterpret channel parameter list after modification.
Parameter | %1: | Error value [-]
Incorrect channel parameters as string.
Error type | 1, Error message from NC program.