# ID 294017

Drive error No. 71.
Description | The DSE drive reports error No.71.
Response | Class | 7 | Stop the axis. All active commands inhibited.
Solution | Class | 6 | Contact the service personnel. Eliminate error. Reset the error on the DSE module.
Parameter | %1: |
Logical axis number P-AXIS-00016 of axis affected.
%2: |
DSE drive address.
%3: |
DSE error id.
Error type | 11, Error message from position controller.