# Refreshing tool data (#TOOL REFRESH)

The following command is provided re repeat the inclusion of active tool data, for example in additional axes after an axis exchange in 2.5D mode or to update kinematic-related offset data in channel or tool parameters for an active kinematic.

Syntax:
#TOOL REFRESH | Refresh data of active tool

The command results in the immediate inclusion of the already available data of the active tool. No more tool data is adopted from an internal tool list [5] or requested from an external tool management function. The D word reprogramming function can be deselected.