# ID 120486

Motion path leaves work area.
Description | Start point or target point of programmed movement path is out of active workspace. A workspace must not be left from a tool centre point. A work area can consist of an circular or polygonal area with constant third plane. See also FCT-C14.
Response | Class | 2 | Stop all axes immediately
Solution | Class | 6 | Dependence defined, activated work spaces
Parameter | %1: | Logical axis number [-]
Area Id number of left work area.
%2: | Error value [0.1 µm or 0,0001°]
Start point of movement.
%3: | Upper limit value [0.1 µm or 0,0001°]
Target point of movement.
%4: | Current value [0.1 µm or 0,0001°]
Intersection point leaving the work area.
%5: | Current value [0.1 µm or 0,0001°]
Error type | 1, Error message from NC program.