# ID 150047

Axis number is 0 in continuous jog mode.
Description | NC channel is in manual operation mode, and an axis should move in continuous jog mode . To do this, the axis is linked to a key and continuous jog mode is activated for this axis. Therefore, the axis is selected by specifying its logical axis number (P-AXIS-00016).

When the CNC accepts the data, it detects that the logical axis number is 0. This value is not permitted for logical axis numbers.

Response | Class | 1 | Warning
Solution | Class | 1 | Indication of the logical axis number parameterized in the axis machine data record.
Parameter | %1: | Logical axis number [-]
Incorrect logical axis number 0.
Error type | -