# Numerical input

The input field for numerical values is limited by the internal numeric display.

This numeric display allows motion paths in the range of 200 m at a resolution of 0.1 µm.

By changing the internal conversion factors in a specification file, the input of positions, feeds, etc., may also be used in different units than mm or inch.

## Example

Numerical values as integers or decimal point inputs:

- Decimals are generally separated by a ".” whereby leading zeroes may be omitted.
- Depending on the configuration and programming, inputs for lengths and position values are given in millimetres or inches; angles are entered in degrees [°] or gons [gon].

Input format:

Values: [µm] | Inputs: [mm]
--- | ---
0,1 | 0.0001 or .0001
1 | 0.001 or .001
10 | 0.01 or .01
100 | 0.1 or .1
1000 | 1.0 or .1
10000 | 10.0 or .10
100000 | 100.0 or .100
1000000 | 1000.0 or .1000

## Example

Numerical inputs as hexadecimal numbers:

- These numbers are enclosed in '...' and start with the character combination 16#, 0x or alternatively H. Following leading zeros or blanks are ignored.
- The characters A to F or a to f can be used for an additional six numerals.

Format:'16#<A...F, a..f, 0..9>' oder '0x<A...F, a..f, 0..9>'or 'H<A...F, a..f, 0..9>'

Input format:

'16#FA1B' | is equivalent to decimal value 64027
'0x0ED2' | is equivalent to decimal value 3794
'H1869f' | is equivalent to decimal value 99999

## Example

Numerical inputs as binary numbers (dual numbers):

- These numbers are enclosed in '...' and start with the character combination 2#, 02# or alternatively B. Following leading zeros or blanks are ignored.
- The two digits are displayed as zero (0) and one (1).

Format: '2#<0..1>' or '02#<0..1>' or 'B<0..1>'

Input format:

'2#1010011' | is equivalent to decimal value 83
'02#010011' | is equivalent to decimal value 19
'B11101010' | is equivalent to decimal value 234

## Example

Numerical inputs as octal numbers:

- These numbers are enclosed in '...' and start with the character combination 8# or 08#. Following leading zeros or blanks are ignored.
- The digits 0 to 7 are used for representation.

Format: '8#<0..7>' or '08#<0..7>'

Input format:

'8#12345' | is equivalent to decimal value 5349
'08#0107302' | is equivalent to decimal value 36546