# Compensation value for acceleration in positive motion direction (P-COMP-00087)

P-COMP-00087 | Compensation value for acceleration in positive motion direction
Description | Compensation value at position i for acceleration in positive motion direction.
Parameter | kw.crosstalk.position[i].correction_accelerate_dir_pos
Data type | SGN64
Data range | MIN(SGN64) ≤ P-COMP-00087 < MAX(SGN64)
Axis types | T
Dimension | T: [0.1 µm] | R, S: -
Default value | 0
Remarks | Parameter available as of V3.1.3081.2 and V3.1.3108.4