# ID 70311

Activation of leadscrew error compensation not possible since compensation table is invalid.
Description | Could not activate leadscrew error compensation since no compensation value table exists or it contains errors. See also: [FCT-C5// Section: Leadscrew error compensation] [COMP// Section: Leadscrew error compensation]
Response | Class | 7 | Stop of axis, lead screw error compensation remains inactive
Solution | Class | 6 | Correct compensation table]
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
Error type | 11, Error message from position controller.