# Effectiveness of parameters

## System parameters for homing:

| Measuring system type
| Not absolute | absolute
| Only cam | only zero pulse | Cam and zero pulse |
| I | II | III | IV
ref_ohne_nocken | 0 | 1 | 0 | -
homing_without_zero_pulse | 1 | 0 | 0 | -
abs_pos_gueltig | 0 | 0 | 0 | 1
cam_direct_access | 0 | - | 0 | -
cam_level | X | - | X | -

## Effective parameters with individual homing modes

| Measuring system type
| Not absolute | absolute
| Only cam | only zero pulse | Cam and zero pulse |
| I | II | III | IV
ref_ohne_rev | X | X | X | -
ref_richt | X | X | X | -
fast_from_cam | X | - | X | -
pos_refpkt | X | X | X | -
rpf_weg_bis_nip (simulation) | - | X | X | -
vb_reflow | X | X | X | -
vb_refmax | X | - | X | -