# ID 20999

Invalid weighting of ramp time.
Description | The ramp time weighting programmed with G133/G134 is negative. [PROG// Section: Ramp time weighting (G132/G133/G134)] Example: Wrong: N10 G00 X0 Y0 Z0

N20 G133 = -60 (alternatively: G133 –60)

:

N1000 M30

Correct:

N10 G00 X0 Y0 Z0

N20 G133 = 60 (alternatively: G133 60)

:

N1000 M30

Response | Class | 1 | Continue NC program processing.
Solution | Class | 1 | In the event of a conflict, ramp time weighting is automatically set to 100%, and NC program processing is continued. Before the next program start, a meaningful value greater than zero (nil) should be programmed.
Parameter | %1: | Error value [µs]
Incorrect weighting of ramp time
%2: | Corrected value [-]
Automatically corrected value of weighting of ramp time
Error type | 1, Error message from NC program.