# Axis release after Reset (P-CHAN-00075)

P-CHAN-00075 | Axis release after reset
Description | This parameter defines whether all axes of a channel are released to axis management at RESET.
Parameter | reset_no_axis_to_axv
Data type | BOOLEAN
Data range | 0: All axes are released to axis management at reset (default). 1: All axes remain in the channel at reset.
Dimension | ----
Default value | 0
Remarks | See also P-AXIS-00251