# ID 120215

Stroke of probe (P-AXIS-00086) is 0.
Description | If the measuring function G100 is used, certain measurement types can check and include the stroke of the measuring probe P-AXIS-00086 during the measurement run. In this case, this parameter must be assigned in the MDS. The path velocity is then reduced during the measurement run to such an extent that it can be stopped within the probe stroke after the measuring probe has responded.

For detailed information on measuring function G100, see
FCT-C4// Section: Introduction
[PROG// Section: Measuring functions].

Response | Class | 2 | Program abort.
Solution | Class | 6 | Set MDS parameter P-AXIS-00086 according to the permissible stroke of the measuring probe.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
Error type | 2, Error message on data transfer of parameter lists to controller.