# Error reaction with measurement type 7 (P-CHAN-00266)

P-CHAN-00266 | Error reaction with measurement type 7
Description | With measurement type 7 (measuring with motion to fixed stop), this parameter influences the error response when the fixed stop is not detected in the measurement block. If no error message is output when the fixed stop is not found, the CNC still goes to the position of the current axis actual value at the end of the measurement travel in order to eliminate a possible position lag (e.g. if the specified position lag is not reached completely).
Parameter | meas_fixed_stop_no_error
Data type | BOOLEAN
Data range | 0: Output of an error message if the fixed stop is not detected (default). 1: No output of an error message if the fixed stop is not detected.
Dimension | ----
Default value | 0
Remarks | Parameterisation example: meas_fixed_stop_no_error 1