# ID 110522

CNC controlled homing with zero pulse search in the drive is not supported for spindles.
Description | The use of P-AXIS-00386 in connection with spindles or SAIs (single-axis interpolators) is currently not possible.
Response | Class | 1 | Error message output, P-AXIS-00386 is disabled.
Solution | Class | 1 | Set P-AXIS-00386 to zero.
Parameter | %1: | Logical axis number [-]
Log. Axis number (see also P-AXIS-00016).
%2: | Current value [-]
Value of P-AXIS-00018.
%3: | Current value [-]
Value of P-AXIS-00250.
%4: | Incorrect value [-]
Value of P-AXIS-00386.
%5: | Corrected value [-]
Corrected value of P-AXIS-00386.
Error type | 2, Error message on data transfer of parameter lists to controller.