# ID 120390

Negative software limit switch exceeded.
Description | In HSC mode, the negative software limit switch will be exceeded in programmed contour. The affected contour element is not processed. All previous blocks up to detected contour element are moved. The position of the software limit switch is defined by parameter P-AXIS-00177 and can be changed in the NC program by G98.

See also
[PROG// Section: Setting the negative software limit switch]
[FCT-A2// Section: Description].

Response | Class | 2 | Program execution stop.
Solution | Class | 6 | Check CNC program and offsets, contour programming inside software limits.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis.
%2: | Current value [0.1 µm or 0,0001°]
Current axis position.
%3: | Lower limit value [0.1 µm or 0,0001°]
Negative software limit switch P-AXIS-00177.
Error type | 1, Error message from NC program.