# ID 60172

CamIn: table type does not fit to the selected Cam Interpolation type
Description | A curve synchronization (block MC_CamIn) was commanded via the PLC, whereby the interpolation rule passed in input table_fkt_type does not match the type of the curve table selected with input CamTableID.
Response | Class | 5 | Abort NC program or PLC module.
Solution | Class | 6 | Changing the interpolation rule in the PLC module MC_CamIn.
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle.
%2: | Current value [-]
Table type
%3: | Current value [-]
Commanded interpolation type.
Error type | -