# ID 120815

Deviation between the defined and actual pre-output position of the M/H function exceeds the permissible tolerance.
Description | Due to a limitation in the microjoint function, an M/H function with a pre-output cannot be output at the required position. The specified tolerance value (P-CHAN-00760) was exceeded for such a deviation from the required position.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Increase tolerance (P-CHAN-00760) if possible. Otherwise, check which limitation obstructs the planned pre-output of the M/H function.
Parameter | %1: | Expected value [0.1 µm]
Specified tolerance value for permitted deviation.
%2: | Current value [0.1 µm]
Current actual deviation.
Error type | 1, Error message from NC program.