# ID 110283

Changing the hardware cam id requires restart of the control.
Description | The parameter P-AXIS-00037 indicating the unique hardware code for cam signals cannot be changed while the CNC kernel is running. The new hardware identification is not transferred; the previous active hardware identification remains valid.
Response | Class | 1 | None.
Solution | Class | 1 | Change the entry P-AXIS-00037 only in configuration mode or when the CNC is disabled.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [-]
Current value of P-AXIS-00037.
%3: | Corrected value [-]
Corrected value of P-AXIS-00037.
Error type | 2, Error message on data transfer of parameter lists to controller.