# ID 14365

Machining direction not allowed for center milling.
Description | Permitted machining directions are 1 to 4.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Deselect centre milling or change the machining direction.
Parameter | %1: | Error value
Affected input parameter @P__.
Error type | 1, error message from the NC program