# Maximum number of measurement records for machine calibration (P-STUP-00185)

P-STUP-00185 | Maximum number of measurement records for machine calibration
Description | This parameter defines the maximum number of measurement records during machine calibration using the ISG calibration cycles. This parameter is used internally by measurement cycles and should only be configured or changed in consultation with ISG.
Parameter | configuration.channel[i].decoder.max_vol_comp_measurement_records
Data type | UNS32
Data range | 0 ... MAX(UNS32)
Dimension | ----
Default value | 0
Remarks | Parameterisation example: A maximum of 50 measurement records are logged. configuration.channel[0].decoder.function FCT_VOL_COMP_COMPUTATION configuration.channel[0].decoder.max_vol_comp_measurement_records 50