# ID 50498

Deceleration path greater than residual path.
Description | With active function Edge bending, after activation of measurement signal via measuring probe, residual path P-CHAN-00030 defined in channel parameter list is reduced. The residual path available of current active channel block at this moment must be greater than P-CHAN-00030.

For more information on edge bending see [PROG// Section: Edge bending (G108)].

Response | Class | 4 | Movement stop.
Solution | Class | 0 | Either reduce the P-CHAN-00030 or increase the programmed residual path so that a distance to go of at least P-CHAN-00030 is available after responding to the measurement signal.
Parameter | %1: | Current value [0.1 µm or 0.0001°]
Residual path available in the programmed measuring block.
%2: | Expected value [0.1 µm or 0.0001°]
Residual path depending on P-CHAN-00030 .
%3: | Current value [0.1 µm or 0.0001°]
Path distance of measurement actual positions and target positions.
%4: | Current value [0.1 µm or 0.0001°]
Channel block path.
Error type | 1, Error message from NC program.