# ID 120736

The definition of the control area base plane requires the specification of two axes.
Description | Normally, the control areas of the work area control function (see [FCT-C14// Description]) refer to the first three Cartesian main axes. If a work or protection area is defined with tracking axes, the base plane must be specified with both axes.

See [PROG// Definition of a control area] and

Example with error:

#CONTROL AREA BEGIN [ID1 PROT POLY MIN_EXCUR=0 MAX_EXCUR=360]

G01 F1000 G90

X2 = 0 (Error 120736)

X2 = 0 Y2=100

X2 = 100 Y2=100

X2 = 100 Y2=0

X2 = 0 Y2=0

#CONTROL AREA END

Corrected example:

#CONTROL AREA BEGIN [ID1 PROT POLY MIN_EXCUR=0 MAX_EXCUR=360]

G01 F1000 G90

X2 = 0 Y2=0

X2 = 0 Y2=100

X2 = 100 Y2=100

X2 = 100 Y2=0

X2 = 0 Y2=0

#CONTROL AREA END

Response | Class | 2 | Abort NC program processing.
Solution | Class | 6 | Check and modify the NC program
Parameter | %1: | Current value [-]
ID of affected workspace or protection space
%2: | Error value [-]
Given axes in the area definition
Error type | 1, Error message from NC program.