# ID 20472

Coupling description may not be changed.
Description | When defining a coupling group, the system detects that this coupling group is still currently active. Example: Wrong: N10 G00 X0 Y0 Z0 N20 #SET AX LINK[1,C=X]

N30 #ENABLE AX LINK[1]

:

N100 #SET AX LINK[1,C=Y]

:

N1000 M30

Correct:

N10 G00 X0 Y0 Z0

N20 #SET AX LINK[1,C=X]

N30 #ENABLE AX LINK[1]

:

N90 #DISABLE AX LINK[1]

N100 #SET AX LINK[1,C=Y]

:

N1000 M30

For further information see [PROG// Section: Programming axis couplings]

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. The active access group must first be deactivated before a new definition can be made.
Parameter | %1: | Error value [-]
Number of the coupling group
Error type | 1, Error message from NC program.