# ID 60019

Programmed feed rate greater than maximum limit.
Description | In the tool parameters, dynamic limits can be defined for a spindle (see also [TOOL// Section: Dynamics and gear data]). These limit values are accepted and, if necessary, the feedrate is adapted to these limit values if a D word (e.g. D17) is programmed in the NC program. After overtaking the tool dynamic parameters a check of the spindle feedrate against the maximum spindle feedrate is done.

This error message is output if the minimum spindle speed in the tool data (P-TOOL-00013) is greater than the maximum permissible axis velocity (P-AXIS-00212).

Response | Class | 1 | Spindle feedrate is limited to parameterized maximum feedrate and the program continues to run.
Solution | Class | 1 | Set the minimum spindle speed in the tool data (P-TOOL-00013) lower than the maximum axis velocity (P-AXIS-00212).
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle
%2: | Current value [1µm/s or 0.001°/s]
Programmed feedrate.
%3: | Limit value [1µm/s or 0.001°/s]
Maximum feedrate.
Error type | 1, Error message from NC program.