# Override with manual mode (P-CHAN-00186)

P-CHAN-00186 | Override with manual mode
Description | The axis or path-specific override acts on the feed rate during incremental or continuous jog mode. In handwheel mode no feed rate override weighting is executed. The current feed rate results from the rotation speed of the handwheel, the parameter setting for resolution and increments per CNC cycle. The nominal feed rate is defined by the axis-specific manual mode parametrisation.

This parameter sets the effective override also for handwheel mode.

Parameter | override_v_handwheel
Data type | BOOLEAN
Data range | 0: No feed rate weighting by override with manual mode (default) 1: Feed rate weighting by override in handwheel mode.
Dimension | ----
Default value | 0
Remarks |